## Fan Controls

#### Radiator Fan Switch A Replacement

10-21

Radiator Fan Switch B Replacement

1. Disconnect the radiator fan switch A connector, then remove the radiator fan switch A (A).

1. Install the radiator fan switch A with a new O-ring (B).

1. Disconnect the radiator fan switch A connector, then remove the radiator fan switch A (A).

1. Install the radiator fan switch A with a new O-ring (B).

a a a