## Honda Multi Matic Transmission/CVT

#### DTC Troubleshooting (cont'd)

14-304

DTC 36: Problem in CVT Speed Sensor Circuit

1. Turn the ignition switch ON (II).
2. Check whether the MIL indicates code for the MAP (manifold absolute pressure) sensor.

Does the MIL indicate code for MAP sensor?

YES - Perform the Troubleshooting Flowchart for the MAP sensor (see page 11-59). Recheck for DTC 36 after troubleshooting.

NO - Go to step 3.

3. Turn the ignition switch OFF.
4. Disconnect CVT speed sensor connector.
5. Turn the ignition switch ON (II).
6. Measure the voltage between CVT speed sensor connector terminal No. 1 and body ground.

CVT SPEED SENSOR CONNECTOR

Wire side of female terminals

Is there about 5 V?

YES - Go to step 7.

NO - Go to step 13.

7. Turn the ignition switch OFF.

8. Check for continuity between CVT speed sensor connector terminal No. 2 and body ground.

CVT SPEED SENSOR CONNECTOR

Wire side of female terminals

Is there continuity?

YES - Repair short to ground in the wire between PCM connector terminal C22 and the CVT speed sensor.

NO - Go to step 9.

9. Check for continuity between CVT speed sensor connector terminal No. 3 and body ground.

CVT SPEED SENSOR CONNECTOR

Wire side of female terminals

Is there continuity?

YES - Go to step 10.

NO - Repair loose connector or open in the wire between the CVT speed sensor connector terminal No. 3 and ground (G101), or repair poor ground (G101).