## Side Sill Outer Panel

#### Removal

3-3

- Cut and pry off the side sill outer panel.
- Check the centre pillar stiffener lower and side sill reinforcement position and check for damage. If necessary, replace the side sill reinforcement.
- Replace the driver's side sill reinforcement as an assembly because of the way the stiffener is attached inside the side sill reinforcement.

1. OUTER PANEL
2. SIDE SILL REINFORCEMENT
3. REINFORCEMENT STIFFENER (Driver side)
4. INSIDE SILL
5. INSIDE SILL EXTENSION
6. CENTRE INNER PILLAR
7. SIDE SILL REINFORCEMENT
8. VIEW (Z)
9. CENTRE PILLAR STIFFENER LOWER
10. WHEEL ARCH EXTENSION
11. SIDE SILL REINFORCEMENT
12. OUTER PANEL
13. FRONT PILLAR LOWER STIFFENER

a a a