## Seats

#### Front Seat Disassembly/Reassembly - Passenger's

20-232

For some models: SRS components are located in this area. Review the SRS component locations (see page 23-24) and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service.

NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

Disassemble the seat as shown.

Reassemble the seat in the reverse order of disassembly and note these items:

- Apply multipurpose grease to the moving portion of the seat track.
- To prevent wrinkles in the seat cushion cover, stretch the material evenly over the pad.

  1. SEAT HEATER HARNESS

     (For some models)

  2. HOOKS

     (Five places)

  3. HOOKS
  4. Release the seat cushion cover from the cushion frame spring.
  5. HOOK
  6. HEADREST
  7. SEAT-BACK
  8. SIDE AIRBAG HARNESS
  9. HOOK
  10. CLIP
  11. RECLINE COVER
  12. RECLINE KNOB
  13. HOOK
  14. CLIP
  15. CLIP
  16. SEAT HEATER UNIT

      (For some models)

  17. SLIDE LEVER
  18. SEAT CUSHION FRAME/ SEAT TRACKS
  19. CLIP
  20. CLIP
  21. HOOK
  22. CLIP
  23. HANGER SPRING

      (With side airbag)

  24. CENTRE COVER
  25. HOOK
  26. OPDS HARNESS