## Manual Transmission

#### Transmission Reassembly (cont'd)

13-46

13. Install the 8 mm flange bolts finger-tight.

14. Tighten the 8 mm flange bolts in a crisscross pattern in several steps.

15. Remove any dirt and oil from the shift lever cover sealing surface. Apply liquid gasket (P/N 08718-0001) to the sealing surface.

1. Liquid gasket

1. Install the 8 x 10 mm dowel pins (A) and shift lever assembly (B).