## Standards and Service Limits

#### Honda Multi Matic Transmission and HMM Differential (cont'd)

2-26

Item | Measurement | Qualification | Standard or New | Service Limit
Drive pulley shaft | Diameter of needle bearing contact area | Flywheel side | 24.007-24.020 mm (0.945-0.946 in.) | When worn or damaged
Forward clutch side | 24.007-24.020 mm (0.945-0.946 in.) | When worn or damaged
I.D. | at sealing ring | 24.007-24.020 mm (0.945-0.946 in.) | When worn or damaged
Driven pulley shaft | Diameter of needle bearing contact area | Start clutch side | 43.981-43.991 mm (1.7315-1.7319 in.) | When worn or damaged
Thrust clearance | Start clutch side | 0-0.13 mm (0-0.005 in.) | -
Cotter, 25.5 mm thickness (Start clutch hub) | A | 2.90 mm (0.114 in.) | When worn or damaged
B | 3.00 mm (0.118 in.) | When worn or damaged
C | 3.10 mm (0.122 in.) | When worn or damaged
D | 3.20 mm (0.126 in.) | When worn or damaged
Starter clutch feed pipe O.D. | End cover side | 6.97-6.98 mm (0.274-0.275 in.) | 6.95 mm (0.274 in.)
Flywheel housing side | 8.97-8.98 mm (0.353-0.354 in.) | 8.95 mm (0.352 in.)
Driven pulley shaft feed pipe O.D. |  | 11.47-11.48 mm (0.4516-0.4520 in.) | 11.45 mm (0.451 in.)
Start clutch feed pipe bushing I.D. | End cover side | 7.00-7.015 mm (0.2756-0.2762 in.) | 7.030 mm (0.277 in.)
Flywheel housing side | 9.0-9.015 mm (0.354-0.355 in.) | 9.03 mm (0.356 in.)
Driven pulley shaft feed pipe bushing I.D. |  | 11.50-11.518 mm (0.4528-0.4535 in.) | 11.533 mm (0.454 in.)
Start clutch end plate I.D. |  | 88.90-88.935 mm (3.500-3.501 in.) | When worn or damaged
Secondary gear shaft | Thrust clearance |  | 0-0.15 mm (0-0.006 in.) | -
Thrust shim, 25 x 35 mm thickness | A | 2.80 mm (0.110 in.) | When worn or damaged
B | 2.90 mm (0.114 in.) | When worn or damaged
C | 3.00 mm (0.118 in.) | When worn or damaged
D | 3.10 mm (0.122 in.) | When worn or damaged
E | 3.20 mm (0.126 in.) | When worn or damaged
F | 3.30 mm (0.130 in.) | When worn or damaged
G | 3.40 mm (0.134 in.) | When worn or damaged
H | 3.50 mm (0.138 in.) | When worn or damaged
I | 3.60 mm (0.142 in.) | When worn or damaged
J | 3.70 mm (0.146 in.) | When worn or damaged
K | 3.80 mm (0.150 in.) | When worn or damaged
Sealing ring groove width |  | 2.50-2.65 mm (0.098-0.104 in.) | 2.655 mm (0.105 in.)
Park gear and pawl |  |  |  | When worn or damaged

a a a