## Interior Trim

#### Trim Removal/Installation - Tailgate Area

20-209

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown.

Install the trim in the reverse order of removal and replace any damaged clips.

Fastener Locations
A : Clip, 4 | B : Clip, 13 | C : Clip, 2 | D : Hook, 2

1. TAILGATE LOWER TRIM PANEL
2. TAILGATE LOWER TRIM PANEL
3. RIGHT TAILGATE SIDE TRIM
4. TAILGATE UPPER TRIM PANEL
5. TAILGATE UPPER TRIM PANEL
6. TAILGATE SIDE TRIM
7. First pry out here.
8. LEFT TAILGATE SIDE TRIM
9. TAILGATE SIDE TRIM