## Cylinder Head

#### Cylinder Head Installation (cont'd)

6-20

8. Install the timing belt, refer to the '01 Civic Shop Manual on this CD (see page 6-22).
9. Adjust the valve clearance, refer to the '01 Civic Shop Manual on this CD (see page 6-14).
10. Install the cylinder head cover, refer to the '01 Civic Shop Manual on this CD (see page 6-55).
11. Install the intake manifold (A) and tighten the bolts/nuts in a crisscross pattern in 2 or 3 steps, beginning with the inner nut. Always use a new intake manifold gasket (B).

12. Tighten the three bolts (C) securing the intake manifold and brackets.

13. Install the new exhaust manifold gasket (A) and exhaust manifold (B). Loosely install the new nuts, then install the cover (C) and loosely install the new bolts.

14. Tighten the bolts/nuts in a crisscross pattern in 2 or 3 steps.
15. Install the exhaust pipe with a new gasket (D).
16. Install the A/C hose bracket.