## Transmission Housing/Flywheel Housing

#### Flywheel Housing and Start Clutch Removal

14-356

Exploded View

1. ATF PASSAGE LINE HOLDER ASSEMBLY
2. 8 x 1.25 mm BOLTS
3. FLYWHEEL HOUSING
4. FLYWHEEL HOUSING GASKET, Replace
5. O-RING, Replace
6. ATF PASSAGE LINE ASSEMBLY
7. 6 X 1.0 MM BOLT
8. ATF PUMP DRIVE CHAIN
9. SNAP RING
10. THRUST SHIM, 22 x 28 mm

    Selective part

11. 6 x 1.0 mm BOLT
12. ATF PUMP DRIVE SPROCKET
13. PITOT FLANGE
14. ATF PUMP DRIVE SPROCKET HUB
15. THRUST WASHER
16. THRUST NEEDLE BEARING
17. THRUST WASHER
18. INPUT SHAFT
19. TRANSMISSION HOUSING
20. DIFFERENTIAL ASSEMBLY
21. O-RING, Replace
22. DRIVEN PULLEY SHAFT
23. PARK PAWL
24. PARK PAWL SPRING
25. PARK PAWL SHAFT
26. SECONDARY DRIVE GEAR ASSEMBLY
27. SECONDARY DRIVE SHAFT
28. THRUST SHIM, 25 x 35 mm

    Selective part

29. START CLUTCH ASSEMBLY
30. COTTERS, 25.5 mm

    Selective parts

31. COTTER RETAINER
32. O-RING, Replace
33. SNAP RING
34. DOWEL PIN, 3