## Standards and Service Limits

#### Honda Multi Matic Transmission and HMM Differential (cont'd)

2-25

Item | Measurement | Qualification | Standard or New | Service Limit
Input shaft | Diameter of needle bearing contact area | Flywheel side | 19.987-20.000 mm (0.7869-0.7874 in.) | When worn or damaged
Forward clutch side | 19.987-20.000 mm (0.7869-0.7874 in.) | When worn or damaged
Thrust clearance | ATF pump driven sprocket hub | 0.37-0.65 mm (0.015-0.026 in.) | -
Planetary carrier | 0.05-0.11 mm (0.002-0.0043 in.) | -
Feed pipe O.D. | Drive pulley feed pipe | 6.97-6.98 mm (0.274-0.275 in.) | 6.95 mm (0.274 in.)
Forward clutch feed pipe | 11.47-11.48 mm (0.4516-0.4520 in.) | 11.45 mm (0.451 in.)
Feed pipe bushing I.D. | Drive pulley feed pipe | 7.00-7.015 mm (0.2756-0.2762 in.) | 7.030 mm (0.277 in.)
Forward clutch feed pipe | 11.5-11.518 mm (0.4528-0.4535 in.) | 11.533 mm (0.454 in.)
Sealing ring groove width |  | 2.00-2.10 mm (0.079-0.083 in.) | 2.105 mm (0.083 in.)
Thrust shim, 22 x 28 mm thickness (ATF pump driven sprocket hub) | C | 1.15 mm (0.045 in.) | When worn or damaged
D | 1.40 mm (0.055 in.) | When worn or damaged
E | 1.65 mm (0.065 in.) | When worn or damaged
F | 1.90 mm (0.075 in.) | When worn or damaged
G | 2.15 mm (0.085 in.) | When worn or damaged
H | 2.40 mm (0.095 in.) | When worn or damaged
Thrust shim, 25 x 31 mm thickness (Planetary carrier) | A | 1.050 mm (0.041 in.) | When worn or damaged
B | 1.12 mm (0.044 in.) | When worn or damaged
C | 1.19 mm (0.047 in.) | When worn or damaged
D | 1.26 mm (0.050 in.) | When worn or damaged
E | 1.33 mm (0.052 in.) | When worn or damaged
F | 1.40 mm (0.055 in.) | When worn or damaged
G | 1.47 mm (0.058 in.) | When worn or damaged
H | 1.54 mm (0.061 in.) | When worn or damaged
I | 1.61 mm (0.063 in.) | When worn or damaged
J | 1.68 mm (0.066 in.) | When worn or damaged
K | 1.75 mm (0.069 in.) | When worn or damaged
L | 1.82 mm (0.072 in.) | When worn or damaged
M | 1.085 mm (0.0427 in.) | When worn or damaged
N | 1.155 mm (0.0454 in.) | When worn or damaged
O | 1.225 mm (0.0482 in.) | When worn or damaged
P | 1.295 mm (0.0510 in.) | When worn or damaged
Q | 1.365 mm (0.0537 in.) | When worn or damaged
R | 1.435 mm (0.0565 in.) | When worn or damaged
S | 1.505 mm (0.0593 in.) | When worn or damaged
T | 1.575 mm (0.0620 in.) | When worn or damaged
U | 1.645 mm (0.0648 in.) | When worn or damaged
V | 1.715 mm (0.0675 in.) | When worn or damaged
W | 1.785 mm (0.0703 in.) | When worn or damaged

a a a