## Engine Assembly

#### Engine Installation (cont'd)

5-16

34. Install the EVAP canister hose.

35. Install the select cable (A) and shift cable (B) using the plastic washers (C), washers (D) and new cotter pins (E) (M/T).

36. Install the clutch slave cylinder (A) and clutch line bracket mounting bolt (B) (M/T).

37. Install the battery base.
38. Install the intake air duct (A) and ground cable (B).