## Seats

#### Front Seat Armrest Replacement

20-91

For some models: NOTE: Take care not to tear the seams or damage the seat covers.

1. Unzip the armrest cover (A), and pull back the armrest cover.

   Fastener Location
   : Nut, 1

2. Remove the nut, the wave washer (B), and the washer (C), then remove the armrest (D). If necessary, remove the bushings (E) from the armrest.

3. Remove the bolts, then remove the armrest bracket (A).

Fastener Locations
: Bolt, 2

4. Install the armrest in the reverse order of removal.