## Intake Manifold and Exhaust System

#### Turbocharger and Exhaust Manifold Removal (cont'd)

9-5

1. Remove the three bolts securing the oil level gauge pipe, then move the oil level gauge.

1. Remove the turbocharger cover.

1. Remove the exhaust manifold cover.

1. Remove the two bolts (A) securing the EGR pipe, PCV tube (B) and remove the air flow tube assembly (C).

1. Remove the acoustic cover (see step 1 on page 9-2).

a a a