## Automatic Transmission

#### Interlock System - Shift Lock System Circuit Troubleshooting (cont'd)

14-67

6. Turn the ignition switch OFF.
7. Disconnect PCM connectors A (31P) and E (31P).
8. Press the brake pedal and measure the voltage between PCM connector terminals E22 and A23 or A24.

PCM CONNECTORS

Wire side of female terminals

Is there battery voltage?

YES - Release the brake pedal and go to step 9.

NO - Repair open in the wire between PCM connector terminal E22 and the brake pedal position switch.

9. Reconnect PCM connectors A (31P) and E (31P).

10. Remove the shift lever console panel and the shift lever assembly mounting bolts.
11. Remove the D3 switch/shift lock solenoid connector (6P) from the shift lever bracket, then disconnect the connector.
12. Turn the ignition switch ON (ll).
13. Measure the voltage between the No. 1 terminal of the D3 switch/shift lock solenoid connector (6P) and body ground.

D3 SWITCH/SHIFT LOCK SOLENOID CONNECTOR (6P)

Terminal side of female terminals

Is there voltage?

YES - Go to step 14.

NO - Repair open or short in the wire between the No. 1 terminal of the D3 switch/shift lock solenoid connector (6P) and the under-dash fuse/relay box.