## Maintenance Schedule for Normal Conditions

#### (KY Model)

3-8

Listed by Distance/Time

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule on 3-10 and 3-11 do not apply.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 5,000 km (3,000 miles) or 6 months
Replace engine oil filter | Every 10,000 km (6,000 miles) or 6 months
Clean or replace cleaner element | Every 20,000 km (12,000 miles)
Inspect valve clearance | Every 20,000 km (12,000 miles)
Replace fuel filter |  | l |  | l |  | l |  | l |  | l
Replace spark plugs | Every 20,000 km (12,000 miles)
Replace timing belt and inspect water pump |  |  |  |  | l |  |  |  |  | l
Inspect and adjust drive belts |  | l |  | l |  | l |  | l |  | l
Inspect idle speed |  |  | l |  |  | l |  |  | l |
Replace engine coolant | 200,000 km (120,000 miles) or 120 months, thereafter every 100,000 km (60,000 miles) or 60 months
Replace transmission fluid | Manual Transmission |  |  |  |  |  | l |  |  | l |
Automatic Transmission |  |  |  |  |  | l |  |  | l |
Inspect front and rear brakes | Every 100,000 km (60,000 miles) or 6 months
Replace brake fluid | Every 36 months
Check parking brake adjustment | l | l |  | l |  | l |  | l |  | l
Rotate tyre (Check tyre inflation and condition at least once per month) | Every 100,000 km (60,000 miles)
Visually inspect the following items:
Tie rod ends, steering gearbox and boots | Every 10,000 km (6,000 miles) or 6 months
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS) | l | l | l | l | l | l | l | l | l | l
All fluid levels and condition of fluid
Exhaust system
Fuel line and connections