## Manual Transmission

#### Transmission Reassembly (cont'd)

13-34

1. Install the bearing ring.

1. Install the bearing retainer.

NOTE:

Apply LOCTITE 242 to the 7 Torx screws. Use a No.45 Torx bit to tighten the screws.

Torque:

26 Nm (2.6 kgf/m, 19 lbf/ft)

1. Install the reverse idler shaft bolt (A).

Torque:

38 Nm (3.8 kgf/m, 28 lbf/ft)

1. Install the 5th gear needle bearing collar (A) and 5th gear thrust washer (B) together using the special tool with a hammer.

NOTE: Before installing, apply oil to the thrust surfaces and collar.

1. Install the 5th gear needle bearing.

1. Install the output 5th gear.

1. Install the input 5th gear.

NOTE:

- The insert spring set positions should differ for both sides.
- The ends of the insert springs should not interfere with the hub.
- Before installing, apply oil to the output gear thrust surfaces.

1. Install the 5th gear needle bearing collar, 5th block ring and 5th synchroniser assembly with shift fork in its groove and back plate to the output shaft.

1. Align the shift rod (A) and the shift arm (B). Install a new double spring pin (C).

1. Install the 1st/2nd detent plug, 3rd/4th detent plug, 5th detent plug, detent springs and detent balls.

Torque:

25 Nm (2.5 kgf/m, 18 lbf/ft)

1. Install the insert stopper plate.

a a a