## Driveline/Axle

#### Driveshaft Reassembly (cont'd)

16-18
Driveshaft Installation

10. Check the clearance between the closed ear portion of the bands. If the clearance is not within the standard, close the ear portion of the bands further.

1. Install a new set ring onto the set ring groove of the driveshaft.

2. Clean the areas where the driveshaft contacts the differential thoroughly with solvent or carburettor cleaner and dry with compressed air. Insert the inboard end (A) of the driveshaft into the differential (B) until the set ring (C) locks in the groove (D).