## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-100

DTC 11-1: Open or Increased Resistance in Left Side Airbag Inflator (Without OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Turn the ignition switch OFF. Disconnect the battery negative cable and wait for 3 minutes.
4. Disconnect the SLi connector (A) from the left side airbag (B).

5. Connect the special tool (2 ohm) to the SLi connector.

6. Reconnect the battery negative cable.

7. Erase the DTC memory.
8. Read the DTC.

Is DTC 11-1 indicated?

YES - Go to step 9.

NO - Open or increased resistance in the left side airbag inflator; replace the left side airbag.

9. Disconnect the battery negative cable and wait for 3 minutes.
10. Disconnect the SRi connector (A) from the right side airbag (B).

11. Disconnect the U2o connector (A) from the SRS unit (B). Do not disconnect the special tool (2 ohm) from the SLi connector.