## Cylinder Head

#### Valve Clearance Adjustment (cont'd)

6-11

1. If you feel too much or too little drag, loosen the locknut (A) and turn the adjusting screw (B) until the drag on the feeler gauge is correct.

1. Tighten the locknut and recheck the clearance. Repeat the adjustment if necessary.

1. Rotate the crankshaft 180° clockwise (camshaft pulley turns 90°).

1. Check and, if necessary, adjust the valve clearance on No. 3 cylinder.

1. Rotate the crankshaft 180° clockwise (camshaft pulley turns 90°).

1. Check and, if necessary, adjust the valve clearance on No. 4 cylinder.

1. Rotate the crankshaft 180° clockwise (camshaft pulley turns 90°).

1. Check and if necessary, adjust the valve clearance on No. 2 cylinder.

1. Install the cylinder head cover (see page 6-44).

a a a