## Engine Lubrication

#### Engine Oil Replacement

8-5

1. Warm up the engine.

2. Remove the drain bolt (A) and drain the engine oil.

D15Y4, D17A2 (KU, KQ models), D17A5 (KN model) engines:

Except D15Y4, D17A2 (KU, KQ models), D17A5 (KN model) engines:

3. Reinstall the drain bolt with a new washer (B).

4. Refill with the recommended oil (see page 3-2).

Capacity

D15Y4, D17A2 (KU, KQ models), D17A5 (KN model) engines:

3.3 l (3.5 US qt, 2.9 Imp qt) at oil change

3.5 l (3.7 US qt, 3.1 Imp qt) at oil change

including filter

4.2 l (4.4 US qt, 3.7 Imp qt) after engine overhaul

Except D15Y4, D17A2 (KU, KQ models), D17A5 (KN model) engines:

3.0 l (3.2 US qt, 2.6 Imp qt) at oil change

3.2 l (3.4 US qt, 2.8 Imp qt) at oil change

including filter

4.2 l (4.4 US qt, 3.7 Imp qt) after engine overhaul

5. Run the engine for more than 3 minutes then check for oil leakage.