## Doors

#### Door Weatherstrip Replacement

20-12

Door Upper Seal Replacement

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. At the front-pillar, remove the door stop mounting bolt (A).

Fastener Location

A : Bolt, 1B : Clip, 1C : Clip, 17

2. Detach the clips (B, C), then remove the door weatherstrip (D).
3. Install the weatherstrip in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the weatherstrip is installed in the holder (E) securely.
- Apply liquid thread lock to door stop mounting bolt before installation.
- Check for water leaks, refer to the '01 CIVIC Shop Manual, P/N 62S5A00 on this CD (see step 7 on page 20-25).

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. Remove these items:

- Power mirror, as necessary (see page 20-16)
- Door sash trim (see page 20-11)

2. Detach the door weatherstrip clips (A, B), then remove the door upper seal (C).

Fastener Location

A : Clip, 1B : Clip, 2

3. Install the seal in the reverse order of removal and note these items:

- Replace the clip if it is damaged.
- Make sure the upper seal is installed in the holder (D) securely.
- Check for water leaks, refer to the '01 CIVIC Shop Manual, P/N 62S5A00 on this CD (see step 7 on page 20-25).