## Sunroof

#### Switch Test/Replacement

22-157

4-door:

1. Remove the driver's pocket (see page 20-76).
2. Disconnect the 6P connector (A) from the sunroof switch (B) and remove the sunroof switch.

3. Check for continuity between the terminals in each switch position according to the table.

5-door:

1. Remove the spotlight (see page 22-137).
2. Push the sunroof switch (A) out from behind the roof lining.

3. Disconnect the 5P connector (B) from the sunroof switch and remove the sunroof switch.
4. Check for continuity between the terminals in each switch position according to the table.