## Openers

#### Tailgate Handle Replacement

20-268

Tailgate Latch Replacement

NOTE: Put on gloves to protect your hands.

1. Remove the tailgate lower trim panel (see page 20-209).
2. Disconnect the tailgate opener cable (A) from the tailgate handle (B) and remove the nuts.

   Fastener Locations
   : Nut, 2

3. Pull out the tailgate handle (A), then remove it.

4. Install the handle in the reverse order of removal and note these items:

- Make sure the tailgate opener cable is connected securely.
- Make sure the tailgate opens properly.

NOTE: Put on gloves to protect your hands.

With Security Switch

1. Remove the tailgate lower trim panel (see page 20-209).
2. Disconnect the tailgate opener cable from the tailgate handle.
3. Disconnect the tailgate latch switch connector (A) and tailgate actuator connector (B), and detach them from the tailgate.

   Fastener Locations
   : Bolt, 3

4. Remove the bolts and pull the tailgate latch (C) out, then remove it.