## Seats

#### Front Seat Disassembly/Reassembly – Without Manual Height Adjustable

20-90

For some models: SRS components are located in this area. Review the SRS component locations (see page 23-23), and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service.

NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- The right side seat is shown, the left side seat is symmetrical.

Disassemble the seat as shown.

Reassemble the seat in the reverse order of disassembly, and note these items:

- Apply multipurpose grease to the moving portion of the seat track.
- To prevent wrinkles in the seat cushion cover, stretch the material evenly over the pad.

  1. SEAT-BACK
  2. HEADREST
  3. HOOKS
  4. Release the seat cushion cover from the cushion frame spring
  5. HOOKS
  6. HOOKS

     (Five place)

  7. OPDS HARNESS

     (For some passenger's seat with side airbag)

  8. SEAT HEATER HARNESS

     (For some models)

  9. CENTRE COVER
  10. CLIP
  11. SEAT CUSHION FRAME/SEAT TRACKS
  12. SEAT HEATER UNIT

      (For some models)

  13. SLIDE LEVER
  14. CLIP
  15. HOOK
  16. RECLINE KNOB
  17. RECLINE COVER
  18. HOOK
  19. SIDE AIRBAG HARNESS

      (For some models)

  20. CLIP
  21. WIRE TIES
  22. CLIP
  23. HANGER SPRING

      (With side airbag)