## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-144

DTC 15-3: Faulty OPDS Sensor

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Check the connection at the OPDS sensor harness connector and the OPDS unit connector.

Are the connections OK?

YES - Go to step 4.

NO - Reconnect the OPDS sensor harness connector and clear the DTC.

4. Replace the OPDS sensor/seat back foam (see page 20-92), and reinitialise the OPDS system (see page 23-33).
5. Erase the DTC memory.
6. Read the DTC.

Is DTC 15-3 indicated?

YES - Go to step 7.

NO - System is OK.

7. Replace the OPDS unit (see page 23-178) and reinitialise the OPDS system.

8. Erase the DTC memory.
9. Read the DTC.

Is DTC 15-3 indicated?

YES - Replace the SRS unit.

NO - System is OK.