## Power Mirrors

#### Power Mirror Actuator Replacement

22-11

1. Remove the mirror holder and disconnect the mirror defogger connectors*, refer to the '01 Civic Shop Manual on this CD, P/N 62S5A00 (see page 20-35).
   *: With defogger
2. Remove the power mirror, refer to the '01 Civic Shop Manual on this CD, P/N 62S5A00 (see page 20-170).
3. Disconnect the 6P connector (A) from the mirror and record the terminal locations and wire colours.

4. Cut the wire harness with wire cutters, and remove the gasket.
5. Remove the three screws from under the mirror.

6. Remove the three Torx screws using a Torx T10 bit, then remove the actuator (A).

Installation:

7. Route the wire harness (A) of the new actuator through the hole in the bracket.

a a a