## Power Mirrors

#### Power Mirror Switch Test

22-147

1. 4-door: Remove the driver's pocket (see page 20-76), then remove the power. Carefully pry the power mirror switch out (A).
   5-door: Carefully pry the power mirror switch out (A).

2. Disconnect the 13P connector (B) from the switch.

3. Check for continuity between the terminals in each switch position according to the table.

Mirror Switch:

Defogger Switch:

Retract switch: