## Exterior Trim

#### Front Pillar Corner Trim Replacement

20-253

1. Open the front door.

2. Wrap a flat-tip screwdriver with protective tape, and apply protective tape around the body to prevent damage. Carefully insert a flat-tip screwdriver next to the upper clip (A) and detach the clip by prying on the front pillar corner trim (B). Take care not to scratch the body and related parts.

3. Gently slide the trim (B) to release the trim from the lower clips (C).

4. Remove the lower clips from the body.

5. Replace any damaged clips.

6. Install the upper clip (A) and lower clips (C) on the trim (B).

7. Hold the trim (B) up and fit the upper clip (A) and lower clips (C) into the holes in the body, then push on the trim until the clips snap into place.