## Bumpers

#### Rear Bumper Removal/Installation

20-105

NOTE:

- Have an assistant help you when removing and installing the rear bumper.
- Take care not to scratch the rear bumper and body.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Put on gloves to protect your hands.

Remove the rear bumper as shown. LHD with rear fog light is shown, RHD with rear fog light is symmetrical.

Install the bumper in the reverse order of removal, and note these items:

- If equipped, make sure the rear fog light connector is plugged in properly.
- Make sure the rear bumper engages the hooks of the side spacers, side brackets and upper brackets on both sides securely.
- Make sure the side spacers of the rear bumper engage the clips on the body securely.
- Replace any damaged clips.

  Fastener Locations
  A: Bolt, 2 | B : Screw, 2 | C : Screw, 2 or 6 | D: Clip, 2
  1. ABSORBER

     (For some models)

  2. REAR BUMPER BEAM

     (For some models)

  3. UPPER BRACKET
  4. HOOKS
  5. SIDE BRACKET
  6. HOOKS
  7. CLIPS
  8. HOOK

     (Six places)

  9. SIDE SPACER
  10. SIDE SPACER
  11. Without rear splash guard only (both sides)
  12. RIGHT REAR SPLASH GUARD

      (For some models)

  13. REAR BUMPER

      If equipped, disconnect the rear fog light connector.

  14. CAP
  15. REAR FOG LIGHT CONNECTOR

      (For some models)

  16. LEFT REAR SPLASH GUARD

      (For some models)

  17. CAP