## Interior Trim

#### Trim Removal/Installation - Trunk Floor and Side Area

20-208

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown. To remove the trunk side trim panel, remove the trunk side upper trim (see page 20-207).

Install the trim in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the trunk compartment light connector is plugged in properly.

  Fastener Locations
  A : Clip, 2 | B : Clip, 4 (White) | C : Clip, 3 | D : Clip, 2 | E : Clip, 2
  1. TRUNK FLOOR MAT
  2. SPARE TYRE LID
  3. RIGHT TRUNK SIDE SPACER

     (For some models)

  4. JACK COVER
  5. TRUNK COMPARTMENT LIGHT CONNECTOR
  6. RIGHT TRUNK SIDE TRIM PANEL
  7. REAR TRIM PANEL
  8. h. LEFT TRUNK SIDE TRIM PANEL
  9. LEFT TRUNK SIDE SPACER

     (For some models)