## Intake Manifold and Exhaust System

#### Exhaust Manifold Removal and Installation

9-7

1. Remove the VTEC solenoid valve (see page 11-110).

1. Remove the intermediate shaft heat cover (see step 2 on page 16-18).

1. Remove the cover and exhaust manifold bracket, then remove the exhaust manifold.

1. COVER
2. EXHAUST MANIFOLD
3. GASKET

   Replace

4. SELF-LOCKING NUT

   10 x 1.25 mm

   44 Nm (4.5 kgf/m, 33 lbf/ft)

5. 10 x 1.25 mm

   44 Nm (4.5 kgf/m, 33 lbf/ft)

6. 8 x 1.25 mm

   22 Nm (2.2 kgf/m, 16 lbf/ft)

   Replace.

   Tighten the bolts in steps, alternating side-to-side.

7. GASKET

   Replace.

8. WASHER
9. EXHAUST MANIFOLD BRACKET

1. Install the exhaust manifold and tighten the bolts/nuts in a criss-cross pattern in two or three steps, beginning with the inner bolt.

1. Install the other parts in the reverse order of removal.

a a a