## Standards and Service Limits

#### Brakes

2-10

Item | Measurement | Qualification | Standard or New | Service Limit
Parking brake lever | Distance travelled when pulled with 196 N (20 kgf, 44 lbs) of force |  | 7-8 clicks
Brake pedal | Pedal height (carpet removed) |  | 184 mm (7.24 in.)
Free play |  | 0.4-3.0 mm (0.016-0.118 in.)
Master cylinder | Piston-to-pushrod clearance |  | 0-0.4 mm (0-0.02 in.)
Brake disc | Thickness | Front | 24.9-25.1 mm (0.98-0.99 in.) | 23.0 mm (0.91 in.)
Rear | 9.9-10.1 mm (0.390-0.398 in.) | 8.0 mm (0.31 in.)
Runout |  | - | 0.10 mm (0.004 in.)
Parallelism |  | - | 0.015 mm (0.0006 in.)
Brake pads | Thickness Front |  | 11.0-11.7 mm (0.43-0.46 in.) | 1.6 mm (0.06 in.)
Thickness Rear |  | 8.3-9.0 mm (0.33-0.35 in.) | 1.6 mm (0.06 in.)
Brake booster | Characteristics at 196 N (20 kgf, 44 lbf) pedal force | Vacuum kPa (mmHg, inHg) | N (kgf, lbf) | kPa (kgf/cm2, psi)
0 (0, 0) | 98 (10, 22) | 0 (0, 0)
294 (30, 66) | 1360 (13.9, 198)
66.7 (500, 19.7) | 98 (10, 22) | 3600 (36.7, 522)
294 (30, 66) | 8980 (91.5, 1301)

a a a