## Automatic Transmission

#### D3 Switch Replacement

14-78

1. Remove the shift lever assembly (see page 14-79).
2. Remove the A/T gear position indicator panel light socket, then remove the indicator light bulb from the socket.
3. Remove the D3 switch/shift lock solenoid connector (6P) and shift lock solenoid connector (2P), then disconnect the shift lock solenoid connector (2P) (see page 14-82).
4. remove the D3 switch and install the new one.
5. Connect the shift lock solenoid connector (2P) and install it and the D3 switch/shift solenoid connector (6P).
6. Install the shift lever assembly (see page 14-80).