## (Except European Model)

3-8

Listed by Maintenance Item

This maintenance schedule outlines the minimum required maintenance that you should perform to ensure the trouble-free operation of the customer's vehicle. Due to the regional and climatic differences, some additional servicing may be required. Please consult the warranty handbook for a more detailed description.

Service at the indicated distance or time whichever comes first. | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
miles x 1,000 | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Normal Condition | Every 10,000 km (6,000 miles) or 12 months
Severe Condition | Every 5,000 km (3,000 miles) or 6 months
Replace engine oil filter | Normal Condition | Every 20,000 km (12,000 miles) or 12 months
Severe Condition | Every 10,000 km (6,000 miles) or 6 months
Clean or replace air cleaner element | Every 20,000 km (12,000 miles)
Inspect valve clearance | Every 40,000 km (24,000 miles),
Replace fuel filter |  |  |  |  |  |  |  |  |  |
Replace spark plugs | Every 40,000 km (24,000 miles)
Replace timing belt, and inspect auto-tensioner, water pump |  |  |  |  |  |  |  |  |  |
Inspect and adjust drive belts |  |  |  |  |  |  |  |  |  |
Inspect idle speed |  |  |  |  |  |  |  |  |  |
Replace engine coolant | At 200,000 km (120,000 miles) or 120 months, then replace every 100,000 km (60,000 miles) or 60 months
Replace transmission fluid | Manual Transmission | Normal Condition |  |  |  |  |  |  |  |  |  |
Severe Condition |  |  |  |  |  |  |  |  |  |
Automatic Transmission | Normal Condition |  |  |  |  |  |  |  |  |  |
Severe Condition |  |  |  |  |  |  |  |  |  |
CVT | Normal Condition |  |  |  |  |  |  |  |  |  |
Severe Condition |  |  |  |  |  |  |  |  |  |
Inspect front and rear brakes | Every 10,000 km (6,000 miles) or 6 months
Replace brake fluid | Every 36 months
Check parking brake adjustment |  |  |  |  |  |  |  |  |  |
Rotate tyre (Check tyre inflation and condition at least once per month) | Every 10,000 km (6,000 miles)
Visually inspect the following items:
Tie rod ends, steering gearbox and boots | Every 10,000 km (6,000 miles) or 6 months
Suspension components
Driveshaft boots
Brake hoses and lines (including ABS) |  |  |  |  |  |  |  |  |  |
All fluid levels and condition of fluid
Exhaust system
Fuel line and connections

Replace engine oil and oil filter according to the Severe Condition Schedule, if the vehicle is driven under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot conditions over 35°C (95°F).
- Extensive idling or long periods of stop-and-go-driving.
- Trailer towing, driving with a car-top carrier or driving in mountainous conditions.
- Driving on muddy, dusty or de-iced roads.

Replace manual and automatic transmission fluid according to the Severe Condition Schedule, if the vehicle is driven in extremely hot conditions over 35°C (95°F) with extensive idling or long periods of stop-and-go driving.

Replace CVT fluid according to the Severe Condition Schedule, if the vehicle is driven at high speed in high temperatures over 35°C (95°F).

a a a