## Ignition Switch

#### Test

22-83

SRS components are located in this area. Review the SRS component locations (see page 23-23) and precautions and procedures (see page 23-25) in the SRS section before performing repairs or servicing.

1. Remove the dashboard lower cover (see page 20-77)
2. Disconnect the 5P connector from the under-dash fuse/relay box.

3. Check for continuity between the terminals in each switch position according to the table.

4. If the continuity checks do not agree with the table, replace the steering lock assembly (see page 17-12).