## Frame Repair Chart

#### Side View

4-10

Unit: mm (in.) o: Inner diameter | a | For sub-frame o 15 (0.59) | e | For damper mount o 11.5 (0.45)
| b1 | For engine mount o 13 (0.51) | f | Damper centre o 78 (3.07)
| b2 | For engine mount o 13 (0.51) | g | For damper mount o 11.5 (0.45)
| b3 | For engine mount o 13 (0.51) | h | For damper mount o 11.5 (0.45)
| c1 | For transmission mount o 13 (0.51) | I | For sub-frame o 11.5 (0.45)
| c2 | For transmission mount o 13 (0.51) | j | For sub-frame o 11.5 (0.45)
| c3 | For transmission mount o 13 (0.51) | k | Locate hole o 25 (0.98)
| d1 | For transmission mount o 13 (0.51) | l | Locate hole o 50 (1.97)
| d2 | For transmission mount o 13 (0.51)
| d3 | For transmission mount o 13 (0.51)