## Fuel and Emissions Systems

#### DTC Troubleshooting Index (cont'd)

11-8

Scan tool DTC | Honda DTC | Detection Item | Page
DTC | Temporary DTC | DTC (MIL Indication*) | Temporary DTC
P0301 | P0301 | 71-1(71) | T71-1 | No. 1 Cylinder Misfire | (see page 11-80)
P0302 | P0302 | 72-1(72) | T72-1 | No. 2 Cylinder Misfire | (see page 11-80)
P0303 | P0303 | 73-1(73) | T73-1 | No. 3 Cylinder Misfire | (see page 11-80)
P0304 | P0304 | 74-1(74) | T74-1 | No. 4 Cylinder Misfire | (see page 11-80)
P0325 | - | 23-1 (23) | - | Knock Sensor Circuit Malfunction | (see page 11-85)
P0335 | - | 4-1 (4) | - | Crankshaft Position (CKP) Sensor No Signal | (see page 11-88)
P0336 | - | 4-2 (4) | - | Crankshaft Position (CKP) Sensor Intermittent Interruption | (see page 11-88)
P0401 | P0401 | 80-1 (80) | T80-1 | Exhaust Gas Recirculation (EGR) Insufficient Flow | (see page 11-154)
P0420 | P0420 | 67-1 (67) | T67-1 | Catalyst System Efficiency Below Threshold | (see page 11-153)
P0443 | - | 92-4 (92) | - | Evaporative Emission (EVAP) Canister Purge Valve Circuit Malfunction | (see page 11-161)
P0500*3 | - | 17-1 (17) | - | Vehicle Speed Sensor (VSS) Circuit Malfunction | (see page 11-90)
P0501*2 | - | 17-2*2 | - | Vehicle Speed Sensor (VSS) Range/Performance | (see page 11-90)
P0563 | - | 34-2 (34) | - | Engine Control Module (ECM)/Powertrain Control Module (PCM) Power Source Circuit Unexpected Voltage | (see page 11-91)
P0600 | - | 39-1 (39) | - | Serial Communication Link Malfunction | Refer to the Multiplex Control System Troubleshooting (see page 22-273).
P07xx** *2 |  | 70-2 (70)*2 | - | Automatic Transaxle System Malfunction*2 | Refer to the Automatic Transmission DTC Troubleshooting Index
P1107 | - | 13-1 (13) | - | Barometric Pressure (BARO) Sensor Circuit Low Voltage | (see page 11-93)
P1108 | - | 13-2 (13) | - | Barometric Pressure (BARO) Sensor Circuit High Voltage | (see page 11-93)
P1259*1 | - | 22-4 (22)*1 | - | VTEC System Malfunction*1 | (see page 11-94)
P1324 | - | 23-2 (23) | - | Knock Sensor Power Source Circuit Low Voltage | (see page 11-87)

*: | These DTCs will be indicated by the blinking of the MIL when SCS short connector is connected.
**: | The D indicator light and the MIL may come on simultaneously.
*1: | D16W7, D16V1 engines
*2: | A/T
*3: | M/T