## Heating

#### Recirculation Control Motor Circuit Troubleshooting (cont'd)

21-37

5-door Except KE Model

1. Check the No. 14 (10A) fuse in the under-dash fuse/relay box.

Is the fuse OK?

YES - Go to step 2.

NO - Replace the fuse and recheck.

2. Disconnect the recirculation control motor 5P connector.
3. Turn the ignition switch ON (II).
4. Measure the voltage between the No. 5 terminal of the recirculation control motor 5P connector and body ground.

RECIRCULATION CONTROL MOTOR 5P CONNECTOR

Wire side of female terminals

Is there battery voltage?

YES - Go to step 5.

NO - Repair open in the wire between the No. 14 fuse in the under-dash fuse/relay box and the recirculation control motor.

5. Turn the ignition switch OFF.
6. Test the recirculation control motor (see page 21-49).

Is the recirculation control motor OK?

YES - Go to step 7.

NO - Go to step 13.

7. Disconnect the push switch 10P connector.

8. Check for continuity between the No. 5 and No. 6 terminals of the push switch 10P connector and body ground individually.

PUSH SWITCH 10P CONNECTOR

Wire side of female terminals

Is there continuity?

YES - Repair any short to body ground in the wire(s) between the push switch and the recirculation control motor.

NO - Go to step 9.

9. Turn the ignition switch ON (II) and check the same terminals for voltage.

PUSH SWITCH 10P CONNECTOR

Wire side of female terminals

Is there any voltage?

YES - Repair any short to power in the wire(s) between the push switch and the recirculation control motor. This short also damages the push switch. Repair the short to power before replacing the push switch.

NO - Go to step 10.