## Engine Assembly

#### Engine Installation (cont'd)

5-13

14. Install exhaust pipe A/TWC (A): use new gaskets (B) and new self-locking nuts (C). Connect the primary HO2S connector (D) and secondary HO2S connector (E) (Except D17A5 engine).

15. Install the splash shield.

16. Install the front tyres/wheels.
17. Lower the hoist.

18. Install the ATF cooler hoses (A/T).

19. Install the heater hose.