## Fuel Supply System

#### Fuel Tube/Quick-Connect Fittings Installation

11-136

1. Check the contact area (A) of the pipe (B) for dirt and damage, and clean if necessary.

2. Insert a new retainer (A) into the connector (B) if the retainer is damaged, or after

- replacing the fuel rail.
- replacing the fuel feed pipe.
- replacing the fuel pump.
- replacing the fuel filter.
- replacing the fuel gauge sending unit
- removing the retainer from the pipe.

3. Before connecting a new fuel tube/quick-connect fitting assembly (A), remove the old retainer from the mating pipe.