## SRS

#### DTC Troubleshooting - with Side Airbags

23-94

DTC 11-1: Open or Increased Resistance in Driver's Side Airbag Inflator (With OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Turn the ignition switch OFF. Disconnect the battery negative cable and wait for 3 minutes.
4. Disconnect the SDi connector (A) from the driver's side airbag (B).

5. Connect the special tool (2 ohm) to the SDi connector.

6. Reconnect the battery negative cable.

7. Erase the DTC memory.
8. Read the DTC.

Is DTC 11-1 indicated?

YES - Go to step 9.

NO - Open or increased resistance in the driver's side airbag inflator; replace the driver's side airbag.

9. Disconnect the battery negative cable and wait for 3 minutes.
10. Disconnect the SPi connector (A) from the front passenger's side airbag (B).

11. Disconnect the U2o connector (A) from the SRS unit (B). Do not disconnect the special tool (2 ohm) from the SDi connector.