## Manual Transmission

#### Transmission Removal (cont'd)

13-7

1. Raise vehicle and make sure it is securely supported.

1. Drain the transmission fluid. Reinstall the drain bolt using a new washer (see page 13-4).

1. Remove the splash shield.

1. Remove the Three Way Catalytic Converter (TWC) assembly (see step 25 on page 5-6).

1. Remove the driveshafts (see page 16-3).

1. Remove the intermediate shaft (see page 16-18).

1. Remove the front engine mount bracket mounting bolt.

1. Remove the three bolts securing the transmission rear mount.

1. Support the sub-frame with a 4 x 4 x 40 in. piece of wood and a jack.

a a a