## Automatic Transmission

#### Road Test

14-2

Shift Schedule

position

Upshift

Throttle Opening | Unit of Speed | 1st - 2nd | 2nd - 3rd | 3rd - 4th | Lock-up ON
Throttle position sensor voltage: 0.75 V | mph | 9-12 | 19-22 | 29-34 | 14-18
km/h | 15-19 | 30-35 | 47-54 | 23-28
Throttle position sensor voltage: 2.25 V | mph | 22-26 | 42-48 | 60-66 | 68-74
km/h | 36-42 | 68-76 | 96-105 | 110-119
Fully-opened throttle, Throttle position sensor voltage: 4.5 V | mph | 34-40 | 67-76 | 103-114 | 103-114
km/h | 55-63 | 108-121 | 166-183 | 166-183

Downshift

Throttle Opening | Unit of Speed | Lock-up OFF | 4th - 3rd | 3rd - 2nd | 2nd - 1st
Throttle position sensor voltage: 0.5 V | mph | 13-17 | 17-20 | 6-10 (3rd - 1st)
km/h | 21-26 | 27-32 | 10-15 (3rd - 1st)
Fully-opened throttle, Throttle position sensor voltage: 4.5 V | mph | 93-104 | 85-96 | 55-62 | 25-30
km/h | 150-166 | 137-153 | 89-100 | 40-48