## Interior Trim

#### Trim Removal/Installation - Door Area

20-29

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.
- LHD is shown, RHD is symmetrical.

Remove the trim as shown. To remove the door sill trim and centre-pillar upper trim, remove the rear side trim panel as necessary (see page 20-30).

Install the trim in the reverse order of removal and note these items:

- Replace any damaged clips.
- Before installing the anchor bolts, make sure there are no twists or kinks in the belts.

Fastener Locations

A : Clip, 2 B : Clip, 3 C : Clip, 7

(Black) (White)

1. CENTRE PILLAR UPPER TRIM
2. FRONT SEAT BELT UPPER ANCHOR BOLT

   7/16-20 UNF

   32 Nm (3.3 kgf/m, 24 lbf/ft)

3. FRONT PILLAR TRIM
4. DOOR OPENING TRIM
5. UPPER ANCHOR COVER
6. FRONT SIDE CAP
7. KICK PANEL
8. DOOR SILL TRIM
9. FRONT SEAT BELT LOWER ANCHOR BOLTS

   7/16-20 UNF

   32 Nm (3.3 kgf/m, 24 lbf/ft)

10. REAR SIDE TRIM PANEL
11. To body.

a a a