## Climate Control

#### In-car Temperature Sensor Test

21-150
Outside Air Temperature Sensor Replacement

Check for a change in resistance by heating or cooling the sensor with a hair drier. Compare the resistance reading between the No. 1 and No. 2 terminals of the in-car temperature sensor with the specifications shown in the graph; the resistance should be within the specifications.

4-door

1. Release the lock and remove the outside air temperature sensor, then disconnect the 2P connector.

2. Install the sensor in the reverse order of removal.