## Valve Body

#### Valve Bodies and ATF Strainer Installation

14-215

Exploded View

1. LOCK-UP SEPARATOR PLATE
2. LOCK-UP VALVE BODY
3. 6 x 1.0 mm, 7 Bolts
4. ATF FEED PIPE (7-position)
5. DOWEL PIN
6. 6 x 1.0 mm, 1 Bolt
7. DOWEL PIN
8. O-RING, Replace
9. DETENT ARM SHAFT
10. WASHER
11. DETENT ARM
12. CONTROL SHAFT
13. ATF FEED PIPE, 8 x 62 mm
14. ATF FEED PIPE, 8 x 40 mm
15. ATF FEED PIPE, 8 X145 mm
16. 6 x 1.0 mm, 1 Bolt
17. ATF STRAINER
18. 6 x 1.0 mm, 8 Bolts
19. SERVO BODY
20. SERVO SEPARATOR PLATE
21. 6 x 1.0 mm, 3 Bolts
22. SECONDARY VALVE BODY
23. STOP SHAFT BRACKET
24. DOWEL PIN, 8 x 40 mm
25. SECONDARY SEPARATOR PLATE
26. ATF PUMP DRIVE GEAR
27. ATF FEED PIPE, 8 x 118 mm
28. TORQUE CONVERTER HOUSING
29. DOWEL PIN
30. MAIN SEPARATOR PLATE
31. ATF PUMP DRIVEN GEAR
32. ATF PUMP DRIVEN GEAR SHAFT
33. MAIN VALVE BODY
34. 6 x 1.0 mm, 5 Bolts
35. ATF FEED PIPE, 8 x 112 mm
36. STATOR SHAFT STOP
37. STATOR SHAFT
38. ATF FEED PIPE, 8 x 138.8 mm
39. TORQUE CONVERTER CHECK VALVE
40. TORQUE CONVERTER CHECK VALVE SPRING
41. COOLER RELIEF VALVE
42. COOLER RELIEF VALVE SPRING
43. ATF FEED PIPE, 8 x 220 mm, Replace.
44. REGULATOR VALVE BODY