## Cooling System

#### Water Pump and Thermostat Inspection (cont'd)

10-9

Water Pump Removal

1. Drain coolant-collect coolant.

1. Loosen fastening bolts (A) before removing drive-belt (B).

1. Remove drive-belt.

1. Remove the water pump assembly (C) and gasket (D).

Water Pump Installation

1. Install the water pump assembly (A) with a new gasket (B) to the cylinder block.

1. Tighten fastening bolts (C) to the specified torque.

Tightening Torque:

24 Nm (2.4 kgf/m, 17.4 lbf/ft).

1. Install the water pump pulley (D) to the water pump. Install the drive-belt (E).

1. Tighten fastening bolts (F) to the specified torque.

Tightening Torque:

9.8 Nm (1.0 kgf/m, 7.2 lbf/ft).

a a a