## Glass

#### Rear Window Replacement (cont'd)

20-185

15. With a sponge, apply a light coat of body primer to the original adhesive remaining around the rear window opening flange. Let the body primer dry for at least 10 minutes:

- Do not apply glass primer to the body and be careful not to mix up glass and body primer sponges.
- Never touch the primed surfaces with your hands.

Hatched area: Apply body primer here

16. Before filling a cartridge, cut a ''V'' in the end of the nozzle (A) as shown.

17. Pack adhesive into the cartridge without air pockets to ensure continuous delivery. Put the cartridge in a caulking gun and run a bead of adhesive (A) around the edge of the rear window (B) as shown.

With the printed dots (C) on the rear window as a guide, apply the adhesive to both side portions of the rear window.

Apply the adhesive within 30 minutes after applying the glass primer. Make a slightly thicker bead at each corner.