## Engine Assembly

#### Engine Installation (cont'd)

5-15

1. Connect the ECM connectors (A) and main wire harness connector (B).

LHD models:

RHD models:

1. Install the throttle cable (see page 11-128), then adjust the cable (see page 11-127).

1. Install the brake booster vacuum hose (A) and the EVAP canister hose (B).

1. Install the fuel feed hose (see page 11-121).

1. Install the select cable (A) and shift cable (B) using the plastic washers (C), washers (D), and new cotter pins (E).

a a a