## Honda Multi Matic Transmission/CVT

#### ATF Cooler Hoses Replacement

14-338

ATF Filter Installation

1. Connect the ATF cooler inlet hose (A) to the cooler inlet line (B) with facing the dot (C) on the hose to the dipstick (D).

2. Connect the inlet hose to the ATF filter (E) until its end aligns with the white line (F).
3. Connect the cooler hoses to the line, ATF filter and ATF cooler and secure them with the clips (G) as shown.
4. Install the cooler hose clamp (H) on the white line (I) on the cooler inlet hose and clamp the outlet hose.
5. Install the radiator hose/ATF cooler hose clamp (J) on the white line (K) on the cooler inlet hose.

1. Install the ATF filter brackets (A) on the ATF filter (B).

2. Install the ATF filter and bracket on the body.